Landon Leigh

801072367

Video Case 2

1. A cell is defined by the coverage area of a base transceiver station (BTS).
2. There are four subsystems in GSM network: Mobile Station (MS), Base Station Subsystem (BSS), Network Subsystem (NSS), and Operation & Maintenance Subsystem (OMSS).
3. To ensure continuous coverage, each cell overlaps at the borders slightly into the other cells.